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BIO CLEAR 10X
Biological Grease-Trap & Septic Treatment
DESCRIPTION

Bio Clear 10X is a stable liquid containing selected micro-organisms and enzymes that efficiently reduce the wastes typically evacuated into the drainage systems of kitchens and other catering and food processing units. Bio Clear 10X is suitable for maintaining septic tanks, grease traps and complete sewerage treatment systems. 
Bio Clear10x has a two-stage operation. When activated with water the ‘free’ enzymes quickly break down the waste into smaller pieces, which are more accessible to the micro-organisms. This initial degradation immediately improves drain flow-rates and reduces odours. It also enables the various strains of micro-organisms in Bio Clear to quickly continue the degrading process, further reducing the smaller particles of solid waste (such as fat, paper and vegetable trimmings) into liquids and gasses.

[image: image2.jpg]™ BIO-
=] PRODUCTIONS




FEATURES AND BENEFITS


· Degrades grease and solid waste

· Neutral PH of 6.5 – 7.5

· Effective on all types of drains and small-bore pipes

· Maintains septic tanks, grease traps and complete 

sewerage systems

· Reduces odours

· Improves drain flow-rates






· No Harmful chemicals or micro-organisms






TECHNICAL INFORMATION

Bio Clear 10x contains many strains of non-pathogenic 

micro-organisms, typically 50,000,000 per millilitre.

Bio Clear is a tan liquid with a very slight yeast fragrance

PACKAGING - code
BC200

BIO CLEAR
200ML
BC1000

BIO CLEAR
1LTR

BC 5

BIO CLEAR
2 X 5LTR


BC 20

BIO CLEAR
20LTR
STORAGE 

Bio Clear is stable for a minimum of 12 months if stored in it’s original, sealed container, in cool dry conditions, away from direct sunlight. Bio Clear 10X is not classified as harmful or irritant under current legislation guidelines. 
DIRECTIONS 
Shake container well before use
SEPTIC TANK & GREASE TRAP TREATMENT (indication only – seek specific advice) Initial shock dose of 500ml/1000ltr capacity should be poured into the system & flushed with a little water. To establish a biomass, add 100ml/1000ltr capacity daily for 1 week. To maintain Septic Tanks 1ml/100ltr capacity applied daily 
Grease Traps apply 1ml per meal (per day) into waste outlets to the trap i.e. 50 meals/day = 50 ml/day. 
For best results use an automatic dosing system.

Disinfectants, bleach caustic and acid products will adversely effect the biological action of Bio-Clear 10x. Drainage systems cannot be damaged or overdosed by this product.









Authorised Distributor Partner:


Biosolve Environmental (Aust) Pty Ltd


6/381 Thompson Road, North Geelong, Victoria 3215


T: 03-5277-0117  F: 03-5277-3689  


 














